{"text_format":"2","workbook":"xlsx","n_sheets":1,"sheets":["Code & Standard 운영현황"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Code & Standard 운영현황","index":0,"n_rows":22,"n_cols":4,"rows_kept":22,"cut":false,"hidden":false,"merged":[[1,0,1,3],[0,0,0,3]]}
["Code & Standard 운영현황"]
["* 2016년도 실적 수량 : 19종"]
["No","Code & Standard명","분야","발행처"]
[1,"ACI","건축","American Concrete Institute"]
[2,"AISC","건축","American Institute of Steel Construction"]
[3,"API : Refining","자원","American Petroleum Institute"]
[4,"ASCE","건축","American Society of Civil Engineers"]
[5,"ASHRAE","냉/난방, 공조","American Society of Heating, Refrigerating, and Air-Conditioning Engineers"]
[6,"ASME : Boiler and Pressure Vessel Code","기계","American Society of Mechanical Engineers"]
[7,"ASME : Standards","기계","American Society of Mechanical Engineers"]
[8,"ASTM","재료시험","ASTM International"]
[9,"AWS","용접","American Welding Society"]
[10,"BSI","토목/재료","British Standards Institution"]
[11,"HI","수자원","Hydraulic Institute"]
[12,"IEC","전기","International Electotechnical Commision"]
[13,"IEEE","전기","The Institute of Electrical and Electronics Engineers. Inc."]
[14,"ISA","기계","International Society of Automation"]
[15,"NACE","재료","The National Association of Corrosion Engineers"]
[16,"NEMA","기계","National Electrical Manufacturers Association"]
[17,"NFPA : Fire Code","화재/소방","National Fire Protection Association"]
[18,"SSPC","재료","The Society for Protective Coatings"]
[19,"UL","안전","Underwriters Laboratories"]